
Name _______________________ 


Auto 110 ‑Hoses Video Review

1. How often should hoses be replaced?

a. every 4 years

b. every 2 years

c. every year

d. they last forever

2. How often should hoses be inspected?

a. every oil change

b. every 6 months

c. every 2 years

3. Which of the following can cause hose failure?

a. heat

b. oil

c. ozone

d. abrasion

e. all of the above

4. A hose will be more likely to fail if it is ___the exhaust manifold.

a.  above 


b. below

5. If a motor mount is bad, what can happen to a hose?

a. it can be torn

b. it can be pulled off

c. both A and B

6. If a hose is stuck to the radiator outlet, what should you do?

a. cut it with a sharp knife

b. use pliers to twist the hose

c. neither a or b

7. When a new hose is installed, what must be done after a run‑in period?

a. replace it

b. twist it

c. retighten the clamp

8. What is the name of a hose that can be formed to fit around a 90( bend?

a. shape 'n fit

b. 90( molded hose

9. Which hose is resistant to ozone?

a. NBR

b. EPDM

10.  Attach the hose to the ______first.

a. engine

b. radiator

