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Auto 110 V-Ribbed Belts Quiz

V-Ribbed Belts

1. V-Ribbed belts were first used in cars in _______________.

a. 1965

b. 1979

c. 1984

d. None of the above

2. V-Ribbed belts can drive accessories using either side of the belt.

True or False?

3. V-ribbed belts are always serpentine.

True or False?

4. Serpentine belts are always V-Ribbed?

True or False?

5. V-Ribbed belts can be inspected while still on the pulleys.

True or False?

6. Most cars that use V-Ribbed belts have a belt routing diagram under the hood.

True or False?

7. Most serpentine belt drives use a spring – loaded belt tensioner.

True or False?

8. Small random cracks are a result of normal wear.

True or False?

9. Multiple cracking or rib chunking is acceptable belt wear.

True or False?

10. Surface finish of the pulley groove is more important with conventional V-belts than with V-ribbed belts.

True or False?

11. Correct alignment of the pulleys is very important to V-ribbed belts, but is very difficult to diagnois.

True or False?

12. Check and re-adjust belt tension after running the engine.

True or False?

13. Standard belt tension gauges do not work properly with V-ribbed belts.

True or False?

14. Tension should be _____ pounds per belt rib on a used belt.

a. 15-20

b. 30

c. 10

15. Tension should be _____ pounds per rib on a new belt.

a. 15-20

b. 30

c. 10

