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AERA Engine Installation Video Review Questions

1. Which of the following could cause a new engine to fail in the same manner as the old one?

1. a defective fuel injector

1. a pinched transmission oil cooler line

1. vacuum leaks from a defective manifold seal

1. all of the above

D
2. Most long blocks include necessary gaskets T/F

true
3. What could result if the flywheel bolts are not torqued correctly?

3. the engine won’t start

3. the rear seal could leak

3. the engine will not turn over

3. all of the above

3. none of the above

B
4. If an engine has had bearing failure, which of the following precautions should be observed?

4. replace the oil pump screen

4. remove all oil gallery plugs and clean with a rifle brush

A/B
5. If the air conditioning compressor seal if defective, where might oil be found?

On the underside of the hood
6. What does the film recommend to do to a thermostat to help it bleed air?

Drill a hole in it
7. A serpentine belt will often result in a water pump that turns backwards from one with an ordinary v-belt.  T/F

true
8. What is used when installing a clutch disk to a flywheel?

A pilot tool
9. Which are ways that the cooling system can be bled of air?

9. through the bleed valve

9. through the highest heater hose

A/B
10. Which are acceptable ways of priming the lubrication system?

10. crank the engine with the fuel and ignition disabled

10. use  pressure primer

B
11. If the engine doesn’t start in 20 seconds, what do you do?

Stop cranking
12. Oil pressure that drops slightly at idle is normal. T/F

True
13. Require the customer to return at _____ miles.           

500

