                                                                              Name                                                   
Preparing the Head for Machining

1. What is the purpose of a valve rotator?

2. What are two things that are easily lost when cleaning a cylinder head?

2. valve tip caps

2. valve shims

2. rocker arm studs

2. all of the above

3. The maximum amount to grind off of a stem tip is 0.                “.
4. What is the purpose of a sodium filled valve stem?

5. What happens if sodium contacts water?

6. The maximum amount of warp in a 6" length is 0.                   “.
7. Which of the following methods can be used to change valve spring tension?

7. Valve shims

7. Valve spring inserts (VSI).

7. Special valve locks (keepers)

7. All of the above

8. A tool that tells you if something is the correct size is called a go-    -       gauge.

9. Induction hardened valve seats are hardened to a depth of about 0.                 “.
10. Surfacing a(n) (OHC/pushrod: circle one) head causes valve timing to retard.

11. Surfacing a head causes _____________ in compression ratio.

11. An increase

11. A decrease

11. No change

12. If a spring is out of square more than 5/64" at a length of        “ it should be discarded.
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