Key


Preparing the Head for Machining

1. What is the purpose of a valve rotator?

To help cool the valve

2. What are two things that are easily lost when cleaning a cylinder head?

2. valve tip caps

2. valve shims

2. rocker arm studs

2. all of the above

a/b

3. The maximum amount to grind off of a stem tip is 0. 030   “.
4. What is the purpose of a sodium filled valve stem? To carry heat from the valve neck to the upper stem and the valve guide

5. The maximum amount of warp in a 6" length is 0. 002  “.
6. Which of the following methods can be used to change valve spring tension?

6. Valve shims

6. Valve spring inserts (VSI).

6. Special valve locks (keepers)

d. All of the above

7. A tool that tells you if something is the correct size is called a go-no  - go    gauge.

8. Induction hardened valve seats are hardened to a depth of about 0. 030 “.
9. Surfacing a(n) (OHC/pushrod: circle one) head causes valve timing to retard.

10. If a spring is out of square more than 5/64" at a length of   2 “ it should be discarded.
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