
Name                                                        
Auto 111 - Engine Rebuilding 

SAFETY TEST 

LISTNUM ParaNumbers1 \l 1
Because some solvents can irritate skin and cause allergic reactions, it is a good idea to wear                                           when using solvent.



LISTNUM ParaNumbers1 \l 1
Hot tanks use caustic as a cleaner.  It is a good idea to protect eyes and

                             .

LISTNUM ParaNumbers1 \l 1
When using a glass bead cleaner, it is important that the reclaim motor is

               .

LISTNUM ParaNumbers1 \l 1
When using a hydraulic floor jack it is essential that jack                             be used.

LISTNUM ParaNumbers1 \l 1
A jack stand should be used on a           ,                surface.

LISTNUM ParaNumbers1 \l 1
Only a quality type                        should be used to support a car.

LISTNUM ParaNumbers1 \l 1
A creeper should always be stood on          when not in use.

LISTNUM ParaNumbers1 \l 1
When attaching a sling to an engine prior to engine removal, be sure to use 
                 of the proper length.

LISTNUM ParaNumbers1 \l 1
Don't                            on an engine when it is hanging by its sling on a cherry picker.

LISTNUM ParaNumbers1 \l 1
After an engine is removed from a car it is                                to raise the car on a two-post hoist because the car won't be balanced.

LISTNUM ParaNumbers1 \l 1
When raising a car on the                       , raise it a little off the ground and shake it to be sure it is safely placed.

LISTNUM ParaNumbers1 \l 1
When using a hydraulic press, use                        goggles and be especially careful that a part doesn't explode.

LISTNUM ParaNumbers1 \l 1
When mounting an engine on an engine                  be sure the mounting bolts are long enough and that they are tight.

LISTNUM ParaNumbers1 \l 1
Be cautious as a drill starts to break through the piece being                    .  That is when it will have a tendency to get stuck.

LISTNUM ParaNumbers1 \l 1
Be sure the chuck                     is our of the chuck before using a drill press.

LISTNUM ParaNumbers1 \l 1
Be sure any work being drilled is                                to the table.

LISTNUM ParaNumbers1 \l 1
Stand to the                        when starting a grinder because grinding wheels sometimes explode when starting up.

LISTNUM ParaNumbers1 \l 1
Be sure the tool rest on the grinder is positioned close to the                              .

LISTNUM ParaNumbers1 \l 1
When using an air impact wrench be sure to use                                sockets.

LISTNUM ParaNumbers1 \l 1
Be sure not to turn on the impact                          unless it is applied to a bolt, so the socket doesn't come flying off.

LISTNUM ParaNumbers1 \l 1
It is mandatory that                protection is used with drills, grinders, presses, wire wheels, and other pieces of turning machinery.

LISTNUM ParaNumbers1 \l 1
A chisel with a mushroomed             must be reground.

LISTNUM ParaNumbers1 \l 1
The handle of a wrench, ratchet or breaker bar should be                  toward you rather than pushed.

LISTNUM ParaNumbers1 \l 1
A file should have a             installed on the tang.

LISTNUM ParaNumbers1 \l 1
If battery acid comes into contact with your skin or clothing immediately wash the area with _________________.

LISTNUM ParaNumbers1 \l 1
                                                  neutralizes battery acid.

LISTNUM ParaNumbers1 \l 1
A spark near a battery can cause a (an)                                                      .

LISTNUM ParaNumbers1 \l 1
Keep the fill tops off/on (circle one) when charging a battery.

LISTNUM ParaNumbers1 \l 1
The electrical cord should be unplugged before connecting or disconnecting a             charger.

LISTNUM ParaNumbers1 \l 1
The ground/hot:(circle one) cable of a battery should be disconnected first.

LISTNUM ParaNumbers1 \l 1
Disconnect the                                        any time the electrical system is worked on.

LISTNUM ParaNumbers1 \l 1
In case of an electrical fire,                                    the battery immediately in any possible way.

LISTNUM ParaNumbers1 \l 1
Use a                                                      to put out a fuel fire.

LISTNUM ParaNumbers1 \l 1
Do not play with                                    air.

LISTNUM ParaNumbers1 \l 1
Any time you are injured, tell your                                                      .

Date:                                         
Print your name                                                                  
Signature:                                                                             
