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 SEQ CHAPTER \h \r 1Cam Grind Questions – Part One
1. Duration is measured in ___________ degrees.
a. camshaft

b. crankshaft

2. Valve lift affects engine idle.  T/F
3. Duration affects engine idle.  T/F
4. Which of the following test results are affected by duration? (choose any that apply)
a. vacuum test

b. compression test
c. cylinder leakage test
5. When the intake valve closes earlier there is ______________ effective compression ratio?
a. more

b. less

6. Which type of camshaft lobe has a clearance ramp?

a. hydraulic adjustment
b. mechanical adjustment
7. Which of the following is hard on the cam and lifter?

a. excessive valve lash

b. too little valve lash

8. Too little valve lash can result in:
a. a burned valve

b. a rough idle

c. both of the above

9. During which two strokes does valve overlap occur?

10. What effect does more valve overlap have on engine 
a. Idle and low speed operation?
b. High speed operation?
11. What is rocker arm ratio?  Draw a picture.

12. What is a potential problem with using a cam with a high rate of lift?

13. Duration is measured; at

a. .050" lift

b. .006" lift

c. either

14. Should a pushrod engine camshaft be cleaned of its black coating before installing it?

15. Why is the intake valve open before TDC?
16. Why is it still open after BDC?
17. Why does the exhaust valve open before the end of the power stroke, during the blowdown period?
18. Why does the exhaust valve remain open after TDC?
19. Where is the heaviest load between parts in a pushrod flat tappet engine?
20. Why is zddp an important additive in a flat tappet engine?
