Name                                          
          Instructor O.K.                           
HEAD REASSEMBLY SHEET

Fill out this sheet before you reassemble the cylinder head. You can check back on previous assignment sheets to find out the answers to some of these questions. 

Guide repair process performed on the head: (check below)

knurl             thinwall             bronzewall             replacement           
VALVES
How many valves did you grind?           
Intake valves:    Angle              (
Average amount ground from faces:
0.           ​​    “

Average amount ground from stem tips:
 0.               “

Exhaust valves:   Angle              (
Average amount ground from faces?
0.              ” 

Average amount ground from stem tips:
 0.               “

SEAT GRINDING:
Pilot size : 0.                 ”
Stone size and angle :  
intake             ” x              ( exhaust             ”x             (
Width of  45(  seat after 3-angle grind :






intake                       ”   exhaust                    ”
After 30(  grind, measure the seat with dividers :

Distance from top of 45( seat to valve margin   
                    ”

SOLVENT CHECK RESULTS ( prior to spring installation ) :Good           Leaks          
Valve Seat Replacement :   Check any that apply

           a. 
Heads cut to accept a pressed - fit insert

           b. 
Older soft seats replaced so the engine can use unleaded gas.

           c. 
Replace any cracked, burned, or excessively ground seats

Installed Spring Height (of valve spring space before spring installation) : 

  Record measurements below and list the shim size needed.

Intake : ( Example : 1.760    |   .030 )

                               (Height)   (Shim)

              |                              |                              |                 
              |              
Exhaust : (Example : 1.790   |    .060 )

                                 (Height)   (Shim)

              |                               |                              |               

              |                 

Final Installed Height Check   after installation of valves / springs :

Within 0.030" of original measurement?                Yes            No           
41

