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Cylinder Head Review Questions 

1. What would you use to clean grease from engine parts?

1. Acid

1. Base


2. What would you use to clean rust and scale?

2. Acid

2. Base

3. When a bake oven is used to clean a cylinder head or block, what is used to finish the cleaning process? 

3. a shot blaster

3. a tumbler

3. Both

4. Besides checking the warpage of an OHC head on the combustion chamber side, where else would you check it? 

5. What should be done to a warped OHC head with integral cam towers before surfacing it? 

6. Which kind of valve is more likely to suffer keeper groove wear? 

6. One that rotates

6. One that does not rotate

7. When valve springs are lined up and checked with a straightedge, how much shorter than the rest is any of them allowed to be?

7. 1/16"

7. 1/32"

7. 1/8"

8. Which part of the valve should NOT be wire brushed?

8. the neck

8. the stem

c.
the keeper grooves

9. When the valve and seat are ground, which way does the rocker arm tip go?

9. up

9. down

10. How can you compensate for that?


(Over)
11. Which would be done first?

a.
grind the valve seats

b.
repair the valve guides

12. What happens to valve stem height when the valve and seat are ground?

12. Increases

12. Decreases

12. Remains the same

13. When grinding valve seats, which angle can ruin the seat the easiest?

13. 30(
13. 45(
13. 60(
14. How much total indicated runout is allowed on valve seats?

15. Which valve is larger?

15. Intake

15. Exhaust

15. They are the same size

LP11
