Name                                            
AUTO ENGINES

ENGINE “BREAK-IN” QUIZ

To help the valve lifters to “wear-mate” to the cam, you run the engine at a certain RPM for a certain period of time:

1. The RPM is approximately

1. 2000

1. 1000

1. 3000

2. The time is:

2. 20 minutes

2. 1 hour

2. 5 minutes

3. Why is it important to have the ignition timing set and the valve lash adjusted before starting the engine?

3. To ease break-in for the cam and lifters

3. To ease break-in of the bearings

3. To ease break-in of the gaskets

3. All of the above

4. When you first drive the car, how would you attempt to seat the piston rings?

4. Stand on the gas

4. Drive for a long distance on the freeway in second gear



4. Drive at high speed

4. Accelerate and decelerate gently to seat both sides of the rings

5. Describe what you would do to be sure there is adequate oil in all the oil galleries before starting the engine.

6. What is your recommendation for the first oil change and the first filter change?

6. 90 days

6. 6,000 miles

6. 500 miles

Some head gaskets require a certain type of service after the engine has been run a number of times:

7. The service required is                                                                         .

8. The approximate mileage on the engine is                         .

9. Which of the following can be causes of a hot running engine when first started after an overhaul?

9. Retarded timing

9. Disconnected cooling fan sensor

9. Upside down thermostat

9. Restricted radiator

9. All of the above

