AERA Engine Installation Video Review Questions

1. Which of the following could cause a new engine to fail in the same manner as the old one?

a. a defective fuel injector

b. a pinched transmission oil cooler line

c. vacuum leaks from a defective manifold seal

d. all of the above

2. Most long blocks include necessary gaskets T/F

3. What could result if the flywheel bolts are not torqued correctly?

4. If an engine has had bearing failure, which of the following precautions should be observed?

a. replace the oil pump screen

b. remove all oil gallery plugs and clean with a rifle brush

5. If the air conditioning compressor seal if defective, where might oil be found?

6. What does the film recommend to do to a thermostat to help it bleed air?

7. A serpentine belt will often result in a water pump that turns backwards from one with an ordinary v-belt.  T/F

8. What is used when installing a clutch disk to a flywheel?

9. Which are ways that the cooling system can be bled of air?

a. through the bleed valve

b. through the highest heater hose

10. Which are acceptable ways of priming the lubrication system?

a. cranking the engine with the fuel and ignition disabled

b. using a pressure primer

11. If the engine doesn’t start in 20 seconds, what do you do?

12. Oil pressure that drops slightly at idle is normal. T/F

