
Name ________________

Front Wheel Drive Engine and Transaxle Removal Checklist

_______ 1. Disconnect speedometer cable

_______ 2. Disconnect clutch cable (if manual transmission equipped)

_______ 3. Remove front wheels, outer tie rod ends on both sides

_______ 4. Remove ball joint nut. Use puller and pry as necessary to remove ball joint from control arm.

_______ 5. Remove internal CV joint from transmission. Pry or unbolt as needed, depending on axle design.  Repeat for other side.

_______ 6. Disconnect transmission shift linkage.

_______ 7. Remove torque rod, as applicable.

_______ 8. Use an impact wrench to disconnect exhaust pipe from manifold and move it out of the way.

_______ 9. Attach a sling to the engine and transaxle assembly at each side (to allow for balance during engine removal).

_______ 10. Attach an engine hoist to the sling and put a small amount of tension on it, just enough to unload the engine mounts.

_______ 11. Remove the bolts that hold the front engine mount to the cylinder head.. Then remove the mount from the body to allow room for the engine to clear during removal.

_______ 12. Remove the nuts or bolts from the front and rear engine mounts. 

_______ 13. Remove bolts attaching front and rear torque rods to the engine. 

_______ 14. Loosen bolts attaching torque rods to the vehicle body and swing the torque rods to move them out of the way.

_______ 15. Remove the engine. Raise it a few inches and check to be certain that everything has been disconnected.

_______ 16. Removing the engine is best done with two people. One person raises the engine slowly while the other guides it until it clears parts of the vehicle body and frame.

_______ 17. When the engine and transaxle are free of the vehicle, roll the hoist until the engine can be lowered.
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