Name ___________________

Head Disassembly/Inspection Review

1.
When a valve stem is tapered at which end is it smaller, the neck or the stem tip?

2.
When valve stem-to-guide clearance measures 0.008" T.I.R. on a dial indicator, how much actual clearance is there?

3.
How much can a V-6 head be warped?      V-8? 

4.
What is the maximum amount a head can be warped in a 6" length?

5.
Does the hot tank anneal valve springs?

6.
List three things that valve springs are tested for.

7.
What are two types of crack detection that can be used on aluminum? 

8.
When would a crack have the most tendency to leak coolant, when hot or when cold? 

9.
After pinning a crack, what would be done to help to close the crack?

10.
After a crack repair, what type of crack detection technique would you use?
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