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Lower End Review Questions

LISTNUM 1 \l 1
Which of the following can be caused by detonation?

LISTNUM 1 \l 2
ring breakage

LISTNUM 1 \l 2
piston land breakage

LISTNUM 1 \l 2
piston skirt breakage

LISTNUM 1 \l 2
all of the above

LISTNUM 1 \l 1
Which of the following can be caused by preignition?

LISTNUM 1 \l 2 \s 1
burned piston

LISTNUM 1 \l 2
burned spark plug electrode

LISTNUM 1 \l 2
engine overheating

LISTNUM 1 \l 2
a and b only

LISTNUM 1 \l 1
When reboring a cylinder, bore the hole to within        "  of the finished size before honing.

LISTNUM 1 \l 1
After honing a block, clean it thoroughly with 

LISTNUM 1 \l 2 \s 1
gasoline

LISTNUM 1 \l 2
soapy water

LISTNUM 1 \l 2
solvent

LISTNUM 1 \l 2
kerosene

LISTNUM 1 \l 2
any of the above

LISTNUM 1 \l 1
Every 0.001" increase in bore size results in           "  change in the piston ring end gap.

LISTNUM 1 \l 1
Which cam journal is largest, front or rear?  Hint: Which direction is the cam installed from when the engine is in the car?

LISTNUM 1 \l 1
The mark on the ring indicates

LISTNUM 1 \l 2 \s 1
top

LISTNUM 1 \l 2
bottom

LISTNUM 1 \l 2
side

LISTNUM 1 \l 1
What is the amount of minimum piston ring side clearance?

LISTNUM 1 \l 2 \s 1
0.015

LISTNUM 1 \l 2
0.0015

LISTNUM 1 \l 2
0.15

LISTNUM 1 \l 1
When the engine does not respond to additional movement of the accelerator when under load, this is called              .

LISTNUM 1 \l 1
Which is softer, the distributor gear or the cam gear?

LISTNUM 1 \l 1
When a connecting rod bore has a tolerance of 2.1252-2.2527", what size would the first rod produced during a factory shift be? 

LISTNUM 1 \l 2 \s 1
bigger

LISTNUM 1 \l 2
smaller
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