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Piston Ring Review Quiz

1.
Which sides of the piston ring wear?

I. Outside Edge


B.
Inside edge

C.
Top



D. 
Bottom

2.
What is the second ring usually made of?

A.
Cast iron


B.
Moly

C.
Chrome

3.
With which type of ring is it acceptable to "spiral" it onto the piston during installation?

A.
Top compression

B.
2nd compression

C.
Oil ring

4.
Which ring is used for dusty conditions?

A.
Chrome


B.
Moly

C.
Cast iron

5.
Which ring is used as a stock ring for high heat applications?

A.
Chrome


B.
Moly

C.
Cast iron

6.
How far undersize should a cylinder be left after boring and before honing?

A.
.001



B.
.0025

C.
.020



D.
.0002

7.
What is used to clean a block after honing?

A.
Solvent


B.
Kerosene

C.
Soap and water

8.
Too much rod side bearing clearance can increase oil consumption.  

A. True

B. False

9.
How much top ring groove clearance is acceptable?

A.
.008



B.
.004

C.
.001

10.
Where do you position a ring in a worn cylinder bore to check for end gap?

A.
Top



B.
Middle

C.
Below ring travel
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