






Name                                                        
Auto 111 - Engine Rebuilding 

SAFETY TEST 

LISTNUM ParaNumbers1 \l 1
Because some solvents can irritate skin and cause allergic reactions, it is a good idea to protect your                                           when using solvent.


LISTNUM ParaNumbers1 \l 1
Some industrial hot tanks use caustic as a cleaner.  Be sure to protect your eyes and                              .

LISTNUM ParaNumbers1 \l 1
When using a glass bead cleaner, it is important that the electric motor is

on/off (circle one).               . 

LISTNUM ParaNumbers1 \l 1
A jack                             must be used when a vehicle is lifted using a hydraulic floor jack.

LISTNUM ParaNumbers1 \l 1
A jack stand should be used on a           ,                surface.

LISTNUM ParaNumbers1 \l 1
A floor creeper should always be stood on          when not in use.

LISTNUM ParaNumbers1 \l 1
When attaching a sling to an engine prior to engine removal, be sure to use a fastener that extends 1 ½ times its _____________ into the female screw thread.
LISTNUM ParaNumbers1 \l 1
Do not work on an engine that is hanging by its sling on a _________ picker.

LISTNUM ParaNumbers1 \l 1
It is unsafe to raise a vehicle on a two-post hoist after an engine has been removed from a vehicle because the center of _______________ gravity will be offset. 

LISTNUM ParaNumbers1 \l 1
When raising a car on the                       , raise it a little off the ground and shake it to be sure it is safely placed.

LISTNUM ParaNumbers1 \l 1
When using a hydraulic press, use full face protection and be especially careful that a part doesn't ______________.

LISTNUM ParaNumbers1 \l 1
When mounting an engine on an engine stand be sure the mounting bolts are long enough and that they are ________.

LISTNUM ParaNumbers1 \l 1
Be cautious as a drill bit starts to break through the piece being                    .  That is when it will have a tendency to get stuck and break.

LISTNUM ParaNumbers1 \l 1
Be sure the chuck                     is out of the chuck before using a drill press.

LISTNUM ParaNumbers1 \l 1
Be sure any piece of material being drilled is                                to the table.

LISTNUM ParaNumbers1 \l 1
Stand to the                        when starting a grinder because grinding wheels sometimes explode when starting up.

LISTNUM ParaNumbers1 \l 1
Be sure the tool rest on the grinder is positioned close to the                              .


(OVER)

LISTNUM ParaNumbers1 \l 1
When using an air impact wrench be sure to use an                                socket.

LISTNUM ParaNumbers1 \l 1
Be sure not to turn on an impact wrench unless it is applied to a bolt, so the_________ doesn't fly off and take out one of your front teeth.

LISTNUM ParaNumbers1 \l 1
Eye or face protection MUST be used with drills, grinders, presses, wire wheels, and other pieces of ___________ machinery.

LISTNUM ParaNumbers1 \l 1
A chisel with a mushroomed             must be reground.

LISTNUM ParaNumbers1 \l 1
The handle of a wrench, ratchet or breaker bar should be                  toward you rather than pushed.

LISTNUM ParaNumbers1 \l 1
A file should have a             installed on its tang.

LISTNUM ParaNumbers1 \l 1
If battery acid comes into contact with your skin or clothing immediately wash the area with _________________.

LISTNUM ParaNumbers1 \l 1
                                                  neutralizes battery acid.

LISTNUM ParaNumbers1 \l 1
A spark near a battery can cause a (an)                                                      .

LISTNUM ParaNumbers1 \l 1
Keep the fill tops off/on (circle one) when charging a battery.

LISTNUM ParaNumbers1 \l 1
The electrical cord should be unplugged before connecting or disconnecting a             charger.

LISTNUM ParaNumbers1 \l 1
The ground/hot:(circle one) cable of a battery should be disconnected first.

LISTNUM ParaNumbers1 \l 1
Disconnect the                                        any time the electrical system is worked on.

LISTNUM ParaNumbers1 \l 1
In case of an electrical fire,                                    the battery immediately in any possible way.

LISTNUM ParaNumbers1 \l 1
Use a                 extinguisher to put out a fuel fire.

LISTNUM ParaNumbers1 \l 1
Do not play with                                    air.

LISTNUM ParaNumbers1 \l 1
Any time you are injured, tell your                                                      .

Date:                                         
Print your name                                                                  
Signature:                                                                             
