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Cylinder Head Film Review Questions (part two)

1. Which part of the valve should NOT be wire brushed?

2. How deep does metal hardness usually go?

3. When the valve and seat are ground, which way does the rocker arm tip go, up or down?

4. What do you do to compensate for that?

5. Which valve often has a welded on hardened stem tip? Why?

6. When grinding valve seats, which angle can ruin the seat the easiest?

7. What happens if the margin of the valve is too narrow?

8. How do you get seat runout when grinding seats?

9. What is it called when fine compound is used on a valve face and seat with a suction cup?

10. What happens to valve stem height when the valve and seat are ground?

11. How much shorter can one spring be than the rest when lined up and checked with a straightedge?

12. Which valve is larger, intake or exhaust?

