Name_____________

Lower End Assembly Review 


(Part One)
1. If a block has been hot tanked, what must be done to its threaded holes?

2. Do some bearings use dowels instead of locating lugs?

3. What do you do after installing each piston/rod assembly?

4. Which way does the lip on a rubber seal go?

a. Toward the oil

b. Away from the oil

5. If the main cap parting line surface is dirty, what happens to bearing clearance?

a. Becomes more

b. Becomes less


6. When installing main caps, what do you do with a hammer?

7. What do you put on rod bolts when installing rods?

8. If a crank gets nicked, what type of bearing wear results?

9. If an oil pump has a screen that bolts onto it, does the screen require a gasket?

10. Does an oil pump enclosed in an oil pan need a gasket where it bolts onto the block?

11. How do vertical scratches get in the cylinder walls?

Select as many as are true:

a. Air cleaner - change carefully, don’t spill dirt

b. Leaky gaskets

c. Leaky PCV hose 

12. What determines the angle of the crosshatch pattern? 

Select as many as are true:

a. The speed of the drill

b. The speed at which the drill is stroked up and down

