Name______________                                              
Lower End Assembly (Part Two)
1. 
What might cause a ring not to be able to be compressed all the way into a ring groove? 

2. 
Where does the ring seal during combustion, on its top side or its bottom side? 

3. 
What are two bearing properties?

4. 
What part of the core plug should be pounded on during installation, the outside lip or the center?

5. 
Which of the following can happen if the engine and transmission are pulled together with bolts, rather than slipping easily together?   Select as many as are true:

a.     a broken transmission front pump

b.     a bound up pilot bushing

6. 
How do you tell a transmission seal leak from a rear main engine seal leak if the engine and transmission are both dirty and you can’t tell the color or weight of the oil?

7. 
What are two more precautions that should be observed when using silicone?

1. don’t use too much of it

8. 
What are rod “squirt holes” for?

9. 
What bearing property helps it deal with foreign particles?

10. 
What feature of a piston makes it so that it should be installed in only one direction?
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