	
	OK
	Bad

	Mechanical Condition Chassis:
	
	

	Evidence of frame or collision  damage
	
	

	Tire wear/alignment
	
	

	Tires worn?
	
	

	Brake pedal height
	
	

	Brake pedal firmness
	
	

	Front brake linings
	
	

	Rear brake linings
	
	

	Steering wheel freeplay (less than 3”)?
	
	

	Steering linkage
	
	

	Suspension parts:
    springs (ride height
	
	

	Suspension bushings
	
	

	Shock absorbers
	
	

	Rubber snubbers
	
	

	Comments:


	
	

	Power Train:

U-joints, CV joint boots
	
	

	Clutch slippage
	
	

	Clutch freeplay
	
	

	Leaks:
   engine oil
	
	

	Transmission fluid
	
	

	Differential oil
	
	

	Power steering fluid
	
	

	Brake fluid
	
	

	Coolant (appearance-color)
	
	

	Idles smooth:
engine hot
	
	

	Engine cold
	
	

	Transmission  fluid condition
	
	

	Comments:


	
	

	
	OK
	Bad

	Engine:
	
	

	Oil condition (appearance)
	
	

	Oil pressure idling (warm)
	
	

	Lifter noise when cold
	
	

	Vacuum
	
	

	Compression (cranks evenly)
	
	

	Radiator condition
	
	

	Hoses and belts
	
	

	Blow-by (check PCV & air cleaner)
	
	

	Exhaust system condition
	
	

	Oil or soot in tailpipe
	
	

	Exhaust smoke
	
	

	Engine mounts
	
	

	Comments:


	
	

	Electrical system
	
	

	Charging system working
	
	

	Starting system working
	
	

	Battery condition
	
	

	Gauges
	
	

	Radio
	
	

	Lights
	
	

	Heater
	
	

	Wipers
	
	

	Air conditioning
	
	

	Clock
	
	

	Horn
	
	

	Wear and Tear
	
	

	Odometer mileage
	
	

	Owner has file of maintenance records?
	
	

	Tires: all the same brand?
	
	

	Good condition?
	
	


