Valvoline Oil Video review questions:
1. What oil viscosity do most new car owner’s manuals suggest?

 
5W30 or 10W30

2. Which oil viscosity dissipates heat better and allows more power, SAE 5W30 or SAE 20W50?

SAE 5W30

3. What is the current API gasoline motor oil specification? (note: the video is not up to date)

SM

4. What does the C in CG stand for? 

Commercial or Compression Ignition

5. What does the S in SH stand for?

Service Station or Spark Ignition

6. What is currently the best heavy duty diesel oil rating?

CG

7. What approximate percentage of oil is base stock and what percentage is additives? 

Oil is 80% base stock and 20% additives

8.  Oil does not wear out, but ____________ get "overloaded".

Additives

9.  Which of the following are additives found in gasoline engine oil?

Anti-oxidants, corrosion preventers, detergents, E.P.additives, V.I. improvers, pour point depressants, dyes and rust repellants

10.  Old oil and filters should be recycled

11.  What is the API symbol called?

The  "donut"

12.  What is typical new car oil consumption?

3-4,000 miles/qt.

13.  What is the name of the type of oil that is derived from organic compounds with the same additives as regular oil?

Synthetic oil

14.  Do typical manufacturer warranties allow for longer oil change intervals when synthetic oil is used?

No - the warranty could be void if the oil is not changed at the normally specified interval

15.  Antique engines often had 5 horsepower per liter, while newer engines often have ____ h.p. per liter.

80

