Name____________________
Auto 110 Lab Final
Part 3

L.O.F.
Use the repair order on Page 713 of your lab manual to complete this assignment.
Check off each item below for final score (10 points each):
· Lift points correct, no lift pad interference with tires

· Air pressure in tires (install tire air chuck, use tire pressure gauge) 
· Checked air filter on bottom
· Checked for leaks and re-checked oil level
· Used a clean funnel for oil refill
· Fender covers used - no grease on steering wheel or fenders

· Used oil filter placed in oil drain with a hole punched in the top 
· Repair order: neat, clean, and professional including the following:
· oil viscosity
· oil capacity specifications
· obvious problems and future service recommendations
· Door or window sticker with odometer mileage listed
· Clean up counters and floors (greasesweep as needed)
· Clean and return tools.  
