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Crankshaft and Bearings Review Questions
1. You would be most likely to find wear on a thrust bearing on

1. the front thrust face

1. the rear thrust face

2. When a clutch disk wears, pedal free travel becomes

2. more

2. less

2. doesn’t change

3. Which of the following clutch types would not experience a freeplay problem with clutch disk wear?

3. mechanical linkage

3. hydraulic fluid master cylinder

4. Why do you pry on the crankshaft before tightening the thrust bearing cap?

5. What causes a crank journal to wear tapered?

6. What causes a crank journal to wear out of round?

7. When a belt is too tight, which bearing wears?

8. If a 0.010" undersized crankshaft is polished, 0.011" and 0.012" bearing oversizes are available to compensate.  T/F

9. Which of the following can result in an increase in oil consumption?

9. main bearing wear

9. rod bearing wear

10. Which bearing halves suffer wear from dry starts? 

Circle the correct answer(s)

10. Mains: top/bottom

10. Rods:  top/bottom

11. Has oil that is going into the oil pump been filtered yet?

12. A housing bore is 2.257"

The bearing wall thickness is 0.065"

What is the assembled inside diameter of the bearing?                                   
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