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Engine Disassembly Review #2

1. Besides the ring face, where is normal piston ring wear found, on the top or the bottom side?

2. What is the name of the tray that is found in some engines that keeps oil from getting sucked from the sump onto the crankshaft?
3. What is the name of the plate found in some engines that provides support to the main caps and lower end of the block?

4. What is the best way to store a crankshaft, laying down or standing on end?    Why?

5. Which lifter has the greatest load on it as it opens, intake or exhaust?
6. If pushrod engine lifters are to be used again, what precaution must be taken during disassembly?
7. What is the black coating on a camshaft?             Should it be removed before using the cam?
8. What can happen to the inside of a cylinder bore if a core plug is pounded into the water jacket against the outside of a cylinder wall?
9. Where does a cam bearing on a pushrod engine usually wear, top or bottom?
10. While disassembling an engine, how can you tell if a connecting rod is bent?
11. How many average human hairs (0.002") could fit in between the piston skirt and cylinder bore?
12. What is the name of the part used on some engines with timing chains that keeps excess oil from flooding the front crankshaft seal?
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